S

MACHINE STARTS

ACCEPTS THE INPUT

SWITCHING THE MACHINE ON

INDICATION OF PROCESS COMPLETION

ACCEPT THE PAPERS ONE BY ONE

PAPER IS FOLDED

PAPER IS INTERLOCKED WITH A CONNECTING MATERIAL

INPUT PAPER OF DIFFERENT SPECIFIC DIMENSIONS

SIDES FORMATION

BASE FORMATION

STORES THE PAPER BAG

DISPENSES THE PAPER BAG

BAG DISPENSION

PAPER IS INTERLOCKED WITH A CONNECTING MATERIAL

PAPERS ARE FOLDED